In Arduino I add to Library the 8266

Connect Battery, ensure + / -

Connect FTDI to Pins Tx, Rx, and Ground

Turn Switch to Program

Turn On

Push to Code